Nasa ParaWing calculator -Copyright JP Gleyzes 2002-

for detailed information refer to http://freedom2000.free.fr



Nasa ParaWing dimensions (all in cm) :
A =	138,00
B =	92,00
C =	57,16
D =	206,32
E =	149,37
F =	138,00
G =	57,16
H =	12,00
K =	2,30
L =	15,33
M =	12,00
N =	4,00
T =	6,00


Nasa ParaWing surface : 2,85 meter square


Nasa ParaWing standard bridles spacing :
A_A spacing (center panel) =	11,50
B_B spacing (wing edge)    =	22,00
C_C spacing (wing mid)     =	17,00


Nasa ParaWing standard bridles dimensions :
A (center) bridles number =	12
A1 =	153,50	 brake line = 	0
A2 =	170,40	 brake line = 	0
A3 =	171,00	 brake line = 	0
A4 =	170,40	 brake line = 	0
A5 =	169,39	 brake line = 	0
A6 =	168,19	 brake line = 	0
A7 =	167,19	 brake line = 	0
A8 =	166,39	 brake line = 	0
A9 =	166,29	 brake line = 	0
A10 =	166,39	 brake line = 	0
A11 =	157,89	 brake line = 	1
A12 =	152,39	 brake line = 	1

B (wing edge) bridles number =	6
B1 =	161,05	 brake line = 	0
B2 =	156,53	 brake line = 	0
B3 =	150,95	 brake line = 	0
B4 =	144,92	 brake line = 	0
B5 =	137,78	 brake line = 	0
B6 =	129,69	 brake line = 	0

C (wing mid) bridles number =	6
C1 =	165,75	 brake line = 	0
C2 =	162,75	 brake line = 	0
C3 =	160,22	 brake line = 	0
C4 =	157,72	 brake line = 	0
C5 =	147,71	 brake line = 	1
C6 =	139,18	 brake line = 	1


Nasa ParaWing cascade bridles dimensions :
A primary =	88,50
A secondary1 =	65,00	 brake line = 	0
A secondary2 =	81,90	 brake line = 	0
A secondary3 =	82,60	 brake line = 	0
A secondary4 =	82,00	 brake line = 	0
A secondary5 =	81,00	 brake line = 	0
A secondary6 =	79,80	 brake line = 	0
A secondary7 =	78,80	 brake line = 	0
A secondary8 =	78,00	 brake line = 	0
A secondary9 =	77,90	 brake line = 	0
A secondary10 =	78,00	 brake line = 	0
A secondary11 =	69,50	 brake line = 	1
A secondary12 =	64,00	 brake line = 	1

B primary =	88,50
B secondary1 =	73,00	 brake line = 	0
B secondary2 =	68,50	 brake line = 	0
B secondary3 =	63,00	 brake line = 	0
B secondary4 =	57,00	 brake line = 	0
B secondary5 =	50,00	 brake line = 	0
B secondary6 =	42,00	 brake line = 	0

C primary =	88,50
C secondary1 =	77,50	 brake line = 	0
C secondary2 =	74,50	 brake line = 	0
C secondary3 =	72,00	 brake line = 	0
C secondary4 =	69,50	 brake line = 	0
C secondary5 =	59,50	 brake line = 	1
C secondary6 =	51,00	 brake line = 	1
