Nasa ParaWing calculator -Copyright JP Gleyzes 2002-

for detailed information refer to http://freedom2000.free.fr



Nasa ParaWing dimensions (all in cm) :
A =	153.00
B =	102.00
C =	63.37
D =	228.74
E =	165.61
F =	153.00
G =	63.37
H =	13.31
K =	3.37
L =	17.00
M =	12.70
N =	5.51
T =	6.12


Nasa ParaWing surface : 3.50 meter square


Nasa ParaWing standard bridles spacing :
A_A spacing =	12.75
B_B spacing =	25.50
C_C spacing =	22.90


Nasa ParaWing standard bridles dimensions :
A bridles number =	12
A1 =	177.00	 brake line = 	0
A2 =	180.00	 brake line = 	0
A3 =	180.00	 brake line = 	0
A4 =	180.00	 brake line = 	0
A5 =	183.00	 brake line = 	0
A6 =	183.00	 brake line = 	0
A7 =	180.00	 brake line = 	0
A8 =	181.00	 brake line = 	0
A9 =	182.00	 brake line = 	0
A10 =	184.50	 brake line = 	0
A11 =	173.00	 brake line = 	1
A12 =	166.50	 brake line = 	1

B bridles number =	6
B1 =	171.00	 brake line = 	0
B2 =	165.50	 brake line = 	0
B3 =	159.00	 brake line = 	0
B4 =	151.00	 brake line = 	0
B5 =	142.30	 brake line = 	0
B6 =	131.50	 brake line = 	0

C bridles number =	6
C1 =	171.80	 brake line = 	0
C2 =	171.00	 brake line = 	0
C3 =	171.00	 brake line = 	0
C4 =	169.00	 brake line = 	0
C5 =	161.00	 brake line = 	1
C6 =	147.00	 brake line = 	1


Nasa ParaWing cascade bridles dimensions :
A primary =	99.79
A secondary1 =	77.33	 brake line = 	0
A secondary2 =	80.33	 brake line = 	0
A secondary3 =	80.35	 brake line = 	0
A secondary4 =	80.35	 brake line = 	0
A secondary5 =	83.34	 brake line = 	0
A secondary6 =	83.34	 brake line = 	0
A secondary7 =	80.35	 brake line = 	0
A secondary8 =	81.35	 brake line = 	0
A secondary9 =	82.34	 brake line = 	0
A secondary10 =	84.84	 brake line = 	0
A secondary11 =	73.33	 brake line = 	1
A secondary12 =	66.84	 brake line = 	1

B primary =	99.79
B secondary1 =	71.86	 brake line = 	0
B secondary2 =	66.40	 brake line = 	0
B secondary3 =	60.02	 brake line = 	0
B secondary4 =	52.10	 brake line = 	0
B secondary5 =	43.69	 brake line = 	1
B secondary6 =	33.15	 brake line = 	1

C primary =	99.79
C secondary1 =	72.54	 brake line = 	0
C secondary2 =	71.74	 brake line = 	0
C secondary3 =	71.75	 brake line = 	0
C secondary4 =	69.76	 brake line = 	0
C secondary5 =	61.66	 brake line = 	0
C secondary6 =	47.75	 brake line = 	0

