Nasa ParaWing calculator -Copyright JP Gleyzes 2002-

for detailed information refer to http://freedom2000.free.fr



Nasa ParaWing dimensions (all in cm) :
A =	135.00
B =	90.00
C =	55.92
D =	201.84
E =	146.12
F =	135.00
G =	55.92
H =	11.75
K =	2.97
L =	15.00
M =	11.21
N =	4.86
T =	5.40


Nasa ParaWing surface : 2.72 meter square


Nasa ParaWing standard bridles spacing :
A_A spacing (center panel) =	11.25
B_B spacing (wing edge)    =	22.50
C_C spacing (wing mid)     =	24.40


Nasa ParaWing standard bridles dimensions :
A (center) bridles number =	12
A1 =	156.60	 brake line = 	0
A2 =	162.00	 brake line = 	0
A3 =	162.00	 brake line = 	0
A4 =	162.00	 brake line = 	0
A5 =	162.00	 brake line = 	0
A6 =	162.00	 brake line = 	0
A7 =	162.00	 brake line = 	0
A8 =	162.00	 brake line = 	0
A9 =	162.00	 brake line = 	0
A10 =	160.60	 brake line = 	0
A11 =	152.60	 brake line = 	1
A12 =	147.20	 brake line = 	1

B (wing edge) bridles number =	6
B1 =	151.20	 brake line = 	0
B2 =	145.80	 brake line = 	0
B3 =	140.40	 brake line = 	0
B4 =	133.60	 brake line = 	0
B5 =	125.60	 brake line = 	0
B6 =	116.10	 brake line = 	0

C (wing mid) bridles number =	6
C1 =	155.20	 brake line = 	0
C2 =	152.60	 brake line = 	0
C3 =	151.20	 brake line = 	0
C4 =	151.20	 brake line = 	0
C5 =	143.10	 brake line = 	1
C6 =	131.00	 brake line = 	1


Nasa ParaWing cascade bridles dimensions :
A primary =	88.05
A secondary1 =	68.66	 brake line = 	0
A secondary2 =	74.06	 brake line = 	0
A secondary3 =	74.07	 brake line = 	0
A secondary4 =	74.07	 brake line = 	0
A secondary5 =	74.07	 brake line = 	0
A secondary6 =	74.07	 brake line = 	0
A secondary7 =	74.07	 brake line = 	0
A secondary8 =	74.07	 brake line = 	0
A secondary9 =	74.07	 brake line = 	0
A secondary10 =	72.67	 brake line = 	0
A secondary11 =	64.66	 brake line = 	1
A secondary12 =	59.27	 brake line = 	1

B primary =	88.05
B secondary1 =	63.72	 brake line = 	0
B secondary2 =	58.35	 brake line = 	0
B secondary3 =	53.07	 brake line = 	0
B secondary4 =	46.34	 brake line = 	0
B secondary5 =	38.59	 brake line = 	0
B secondary6 =	29.32	 brake line = 	0

C primary =	88.05
C secondary1 =	67.68	 brake line = 	0
C secondary2 =	65.09	 brake line = 	0
C secondary3 =	63.73	 brake line = 	0
C secondary4 =	63.73	 brake line = 	0
C secondary5 =	55.59	 brake line = 	1
C secondary6 =	43.58	 brake line = 	1

