Nasa ParaWing calculator -Copyright JP Gleyzes 2002-

for detailed information refer to http://freedom2000.free.fr



Nasa ParaWing dimensions (all in cm) :
A =	138,00
B =	92,00
C =	57,16
D =	206,32
E =	149,37
F =	138,00
G =	57,16
H =	12,00
K =	2,30
L =	15,33
M =	11,46
N =	4,97
T =	6,00


Nasa ParaWing surface : 2,85 meter square


Nasa ParaWing standard bridles spacing :
A_A spacing (center panel) =	11,50
B_B spacing (wing edge)    =	23,00
C_C spacing (wing mid)     =	19,00


Nasa ParaWing standard bridles dimensions :
A (center) bridles number =	12
A1 =	162,90	 brake line = 	0
A2 =	168,90	 brake line = 	0
A3 =	170,40	 brake line = 	0
A4 =	170,40	 brake line = 	0
A5 =	169,79	 brake line = 	0
A6 =	168,89	 brake line = 	0
A7 =	167,79	 brake line = 	0
A8 =	166,89	 brake line = 	0
A9 =	166,39	 brake line = 	0
A10 =	166,39	 brake line = 	0
A11 =	158,40	 brake line = 	1
A12 =	152,39	 brake line = 	1

B (wing edge) bridles number =	6
B1 =	159,49	 brake line = 	0
B2 =	155,47	 brake line = 	0
B3 =	150,39	 brake line = 	0
B4 =	144,85	 brake line = 	0
B5 =	137,70	 brake line = 	0
B6 =	129,60	 brake line = 	0

C (wing mid) bridles number =	6
C1 =	165,69	 brake line = 	0
C2 =	163,18	 brake line = 	0
C3 =	161,16	 brake line = 	0
C4 =	159,65	 brake line = 	0
C5 =	150,19	 brake line = 	1
C6 =	139,15	 brake line = 	1


Nasa ParaWing cascade bridles dimensions :
A primary =	88,50
A secondary1 =	74,50	 brake line = 	0
A secondary2 =	80,50	 brake line = 	0
A secondary3 =	82,00	 brake line = 	0
A secondary4 =	82,00	 brake line = 	0
A secondary5 =	81,40	 brake line = 	0
A secondary6 =	80,50	 brake line = 	0
A secondary7 =	79,40	 brake line = 	0
A secondary8 =	78,50	 brake line = 	0
A secondary9 =	78,00	 brake line = 	0
A secondary10 =	78,00	 brake line = 	0
A secondary11 =	70,00	 brake line = 	1
A secondary12 =	64,00	 brake line = 	1

B primary =	88,50
B secondary1 =	71,50	 brake line = 	0
B secondary2 =	67,50	 brake line = 	0
B secondary3 =	62,50	 brake line = 	0
B secondary4 =	57,00	 brake line = 	0
B secondary5 =	50,00	 brake line = 	0
B secondary6 =	42,00	 brake line = 	0

C primary =	88,50
C secondary1 =	77,50	 brake line = 	0
C secondary2 =	75,00	 brake line = 	0
C secondary3 =	73,00	 brake line = 	0
C secondary4 =	71,50	 brake line = 	0
C secondary5 =	62,00	 brake line = 	1
C secondary6 =	51,00	 brake line = 	1
