Nasa ParaWing calculator -Copyright JP Gleyzes 2002-

for detailed information refer to http://freedom2000.free.fr



Nasa ParaWing dimensions (all in cm) :
A =	153,00
B =	114,75
C =	63,37
D =	241,50
E =	153,00
F =	153,00
G =	63,37
H =	18,00
K =	3,26
L =	19,13
M =	15,00
N =	0,01
T =	8,50


Nasa ParaWing surface : 3,69 meter square


Nasa ParaWing standard bridles spacing :
A_A spacing (center panel) =	13,00
B_B spacing (wing edge)    =	23,00
C_C spacing (wing mid)     =	19,00


Nasa ParaWing standard bridles dimensions :
A (center) bridles number =	12
A1 =	186,23	 brake line = 	0
A2 =	195,73	 brake line = 	0
A3 =	197,14	 brake line = 	0
A4 =	197,14	 brake line = 	0
A5 =	196,89	 brake line = 	0
A6 =	196,14	 brake line = 	0
A7 =	195,64	 brake line = 	0
A8 =	195,39	 brake line = 	0
A9 =	195,14	 brake line = 	0
A10 =	194,89	 brake line = 	0
A11 =	187,91	 brake line = 	1
A12 =	180,90	 brake line = 	1

B (wing edge) bridles number =	6
B1 =	186,09	 brake line = 	0
B2 =	182,08	 brake line = 	0
B3 =	176,53	 brake line = 	0
B4 =	170,51	 brake line = 	0
B5 =	164,40	 brake line = 	0
B6 =	157,86	 brake line = 	0

C (wing mid) bridles number =	5
C1 =	193,25	 brake line = 	0
C2 =	189,75	 brake line = 	0
C3 =	186,72	 brake line = 	0
C4 =	184,72	 brake line = 	0
C5 =	171,00	 brake line = 	1


Nasa ParaWing cascade bridles dimensions :
A primary =	100,00
A secondary1 =	86,25	 brake line = 	0
A secondary2 =	95,75	 brake line = 	0
A secondary3 =	97,25	 brake line = 	0
A secondary4 =	97,25	 brake line = 	0
A secondary5 =	97,00	 brake line = 	0
A secondary6 =	96,25	 brake line = 	0
A secondary7 =	95,75	 brake line = 	0
A secondary8 =	95,50	 brake line = 	0
A secondary9 =	95,25	 brake line = 	0
A secondary10 =	95,00	 brake line = 	0
A secondary11 =	88,00	 brake line = 	1
A secondary12 =	81,00	 brake line = 	1

B primary =	100,00
B secondary1 =	86,50	 brake line = 	0
B secondary2 =	82,50	 brake line = 	0
B secondary3 =	77,00	 brake line = 	0
B secondary4 =	71,00	 brake line = 	0
B secondary5 =	65,00	 brake line = 	0
B secondary6 =	58,50	 brake line = 	0

C primary =	100,00
C secondary1 =	93,50	 brake line = 	0
C secondary2 =	90,00	 brake line = 	0
C secondary3 =	87,00	 brake line = 	0
C secondary4 =	85,00	 brake line = 	0
C secondary5 =	71,00	 brake line = 	1
